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SCHEDULE C. ZONING DISTRICT DEVELOPMENT STANDARDS[footnoteRef:1] [1: Editor's note(s)—Ord. No. 06O-03-120, § 1, adopted April 10, 2006, amended the title of Schedule C to read as herein set out. Prior to inclusion of said ordinance, Schedule C was entitled, "General Requirements for Building Parcels, Building Setbacks, and Yards, and Area Dimension Regulations for Lot and Tract." ] 

(a)	Residential Districts.
	Land Use Category: 
	RS-4 
	RS-5 
	RM-5 
	RM-8 
	RM-10 
	RM-18 
	RM-22 (15) 
	RM-45 
	RMH-50 
	Unit of Measure- 
ment 

	Minimum Parcel Area Requirement (1) 
	7,500 
	7,000 
	12,000 
	12,000 
	6,500 
single 
family 
12,000 
multi- 
family 
	12,000 
	12,000 
	12,000 
	12,000 
	Sq. Feet 

	Minimum Parcel Frontage on a Street 
	(1) 75 
	(1) 70 
	100 
	100 
	60 single- 
family 
100 multi- 
family 
	100 
	100 
	100 
	20 
	Feet 

	Minimum Building Size (11), (12): 

	Single-Family Detached 
	1,400 
	1,400 
	N/A 
	1,400 
	1,400 
	1,400 
	N/A 
	N/A 
	N/A 
	

	Multi-family, Townhouses and Connected Units 
	
	
	
	
	
	
	
	
	
	

	  Efficiency 
	N/A 
	N/A 
	700 
	700 
	700 
	700 
	700 
	700 
	N/A 
	

	  One Bedroom 
	N/A 
	N/A 
	900 
	900 
	900 
	900 
	900 
	900 
	900 
	

	  Two Bedroom 
	N/A 
	N/A 
	1,000 
	1,000 
	1,000 
	1,000 
	1,000 
	1,000 
	1,000 
	

	  Each Additional Bedroom 
	N/A 
	N/A 
	150 
	150 
	150 
	150 
	150 
	150 
	150 
	

	Setbacks: 
	
	
	
	
	
	(13) 
	
	
	
	

	  Front 
	25 
	25 
	30 
	30 
	30 
	(2) 30 
	(2) 30 
	(2) 30 
	(2) 40 
	Feet 

	  Side 
	7.5 
	7.5 
	20 
	20 
	7.5 single- 
family 
25 multi- 
family (8) 
	(2) 
	(2) 
	(2) 
	(2) 
	Feet 

	  Rear 
	15 
	15 
	15 
	15 
	15 single- 
family 
25 multi- 
family 
	(2) 
	(2) 
	(2) 
	(2) 
	Feet 

	Maximum Lot Coverage 
	40(7) 
	40(7) 
	(4) 
	(7) 
	(9)(7) 
	(5) 
	(5) 
	(5) 
	(5) 
	% of Area Parcel 



	Land Use Category: 
	RS-4 
	RS-5 
	RM-5 
	RM-8 
	RM-10 
	RM-18 
	RM-22 (15) 
	RM-45 
	RMH-50 
	Unit of Measure- 
ment 

	Maximum Building Height (14) 
	2 Story 30 
	2 Story 30 
	2 Story 30 
	3 Story 35 
	2 Story 30 
	8(13) Story 100 
	8 Story 100 
	8 Story 100 
	8 Story 100 
	Stories 
Feet 

	Density-Maximum 
	4 
	5 
	5 
	8 
	10 
	18 
	22 
	45 
	(6) 
	Units Per Acre 



1.	Area and Dimension Regulation Footnotes: 
(1)	Some lots may have a minimum of sixty-six (66) feet of frontage; or 
(2)	One (1) times the building height or greater. 
(3)	Thirty-five (35) percent for two-story buildings; forty (40) percent for one-story buildings. 
(4)	One (1) story = thirty-five (35) percent; 
Two (2) story = thirty (30) percent; 
Three (3) story = thirty (30) percent; 
Four (4) story = twenty-seven (27) percent. 
(5)	One (1) to four (4) story = forty (40) percent; 
Five (5) to eight (8) story = thirty-five (35) percent. 
(6)	One hundred (100) sleeping units per acre or double the maximum density as permitted by the City Future Land Use Map. 
(7)	The maximum lot coverage may be exceeded in cases where an on-site retention system is provided for any runoff generated by the impervious area which is in excess of the maximum allowed in the preceding table. In order to exceed the maximum lot coverage, sealed drawings which set forth the on-site drainage retention must be submitted by an architect, engineer, or landscape architect registered in the State of Florida. The plans must be approved by the City Engineer prior to the issuance of a building permit for the use which causes the need for the on-site retention system. The system must be designed to retain on-site the twenty-five (25) year, three (3) year storm event. In no case shall any lot exceed sixty-five (65) percent lot coverage even when an on-site drainage system is provided. 
(8)	On all corner plots, there shall be a front setback as specified and a side yard at least fifteen (15) feet in width on the side which abuts the side street or dedicated waterway. The front and side of the plot shall be determined from the plat. 
(9)	One (1) story = forty (40) percent; 
Two (2) story = thirty-five (35) percent. 
(10)	Single-family minimum setbacks of fifteen (15) feet rear, twenty-five (25) feet front and seven and one-half (7½) feet side should be applied to single family development in RM-8 zoning districts. 
(11)	The minimum building size refers to living area; it excludes garages, patios, etc. 
(12)	The minimum building size set out above is not applicable to hotels, motels, hospitals, assisted living facilities, dormitories, or special residential facility overlay zones as more particularly described in Schedule U. 
(13)	On all corner plots, there shall be a front setback as specified and a side yard at least ten (10) feet in width on the side that abuts the side street or dedicated walkway. The front and side plot shall be determined from the plat. 
(14)	The maximum building height may be exceeded by up to fifteen (15) feet in order to accommodate unoccupied hierarchical architectural features, such as cupolas and camouflaged telecommunication antenna, designed to create a focal point for the surrounding area. 
(15)	Within the RM-22 zoning district, a one-family dwelling unit shall be subject to the RS-5 zoning district development standards. Alternatively, if located within the RM-22 zoning district and a safe neighborhood district, then the following standards shall be allowed: 
a.	Minimum street frontage: seventy (70) feet. 
b.	Minimum lot depth: eighty-five (85) feet. 
c.	Front setback: twenty (20) feet. 
d.	Rear setback: fifteen (15) feet. 
e.	Side setback: seven and one-half (7½) feet. 
f.	Street side setback: fifteen (15) feet. 
(16)	Recreational amenities and open space. Common open space may be used for amenity or recreation purposes and must be suitably improved for its intended use. Recreational amenities must be ten (10) percent or more of the total square feet dedicated to residential uses. The following amenities shall be provided: 
a.	Swimming pool and associated canopy or recreational water feature if a pool cannot be accommodated; and 
b.	Air-conditioned club house with community conference/meeting room and with restrooms; and 
c.	Playground with playground equipment and canopy shall be provided and incorporated into the overall design scheme of the development; and 
d.	Barbeque areas with canopy; and 
e.	Community gym equipped with weights and cardio equipment. 
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(b)	Non-residential Districts.* 
	
	CO-1 
	C-2 
	C-3 
	C-4 
	I-1 
	CR 
	S-1 
	CF 
	CN 
	Unit of 
Measure- 
ment 

	Land Use Category: 

	Minimum Parcel Area Required 
	No 
Mini- 
mum 
	10,000 
	No 
Mini- 
mum 
	No 
Mini- 
mum 
	No 
Mini- 
mum 
	40,000 
	No 
Mini- 
mum 
	TBD 
	No 
Mini- 
mum 
	Sq. Feet 

	Minimum Parcel Frontage on a Street 
	None 
	100 
	None 
	None 
	None 
	200 
	None 
	TBD 
	None 
	Feet 

	Setbacks: 

	Front 
	25 
	40 
	25 
	25 
	10 
	25 
	25 
	25 
TBD 
	20 
Maxi- 
mum 
	Feet 

	Side, Interior 
	25 
	
	
	
	
	25 
	25 
	TBD 
	0 
	Feet 

	Side, Street 
	
	
	
	
	
	
	
	TBD 
	10 
	Feet 

	Rear 
	205 
	18 
	20 
	20 
	10 
	25 
	25 
	TBD 
	25 
	Feet 

	Maximum Building Area 
	35 
	None 
	None 
	None 
	None 
	None 
	None 
	35 
	25 
	% of 
Parcel 

	Maximum Building Height (9), (11) 
	50 
	75 
	50(10) 
	50 
	50 
	50 
	50 
	100 
	35 
	Feet 

	Maximum District Size 
	
	
	
	
	
	
	
	10,000 
	2 
	Acres 



* The following footnotes apply to this entire Schedule C subsection (b) regarding Non-residential Districts: 
TBD = To Be Determined through the site plan or site plan modification process. 
1.	Area and dimension regulation footnotes: 
(1)	The following setbacks shall be measured from the centerline of the street or parcel which fronts on the following trafficways: 
A.	Commercial Blvd.—One hundred twenty-three (123) feet; 
B.	University Drive—One hundred twenty-five (125) feet; 
C.	Oakland Park Blvd.—One hundred twenty-five (125) feet; 
D.	Sunrise Blvd.—One hundred fifty (150) feet; 
E.	State Road 7—One hundred (100) feet. 
(2)	Required water retention areas may account for only fifty (50) percent of the previous area, when determining amount of open space provided. 
(3)	Where the side or rear property line of non-residential property abuts a residential property line, the side and rear yard setback shall be no less than twenty-five (25) feet. There shall be no parking in the twenty-five (25) feet. Uses found in Schedule B-2 of this Land Development Regulation that require a special exception may be subject to increased setbacks due to the hazards or conflicts inherent with their use, at the discretion of the City Commission. In this 25-foot setback shall be a wall or fence landscaped on both sides with a hedge or vine, and shall include installed shade trees, thirty (30) feet on center. No parking shall be allowed in the twenty-five (25) feet where it abuts residential. 
(4)	When not abutting residential property, the minimum setback shall be five (5) feet on the interior side or one-half (½) times the height of the building, whichever is greater. When not abutting residential property, the minimum rear yard setback shall be a minimum of fifteen (15) feet. 
(5)	When a non-residential property abuts residentially zoned property and is separated from that residentially zoned land by a waterway of at least twenty-five (25) feet, then parking may be allowed in the 25-foot setback, provided that hedging is provided and maintained between the canal and the parking lot and that all other provisions of the landscaping schedule are met. 
(6)	When not abutting a residential district, setback shall be five (5) feet or one-half (½) times the height of the building not to exceed ten (10) feet. 
(7)	Reserved. [See Article III, § 5.34.8 for self-storage facilities setbacks.] 
(8)	Uses found in Schedule B-2 of this Land Development Regulation that require a special exception may be subject to increased height limitations due to the hazards or conflicts inherent with their use, at the discretion of the City Commission. 
(9)	Consistent with the requirements of Article III, Part 5.0, Section 5.41., Telecommunication facility uses, the maximum height for telecommunication antenna support structures is one hundred fifty (150) feet. 
(10)	The height limit in the General Commercial (C-3) zoning district is fifty (50) feet, except that those properties zoned General Commercial district that abut a RS-4, RS-5, or RM-8 zoning district are limited to a maximum building height of twenty-five (25) feet. 
(11)	The maximum building height may be exceeded by up to fifteen (15) feet in order to accommodate unoccupied hierarchical architectural features, such as cupolas and camouflaged telecommunication antenna, designed to create a focal point for the surrounding area. 
(12)	Multifamily developments located in commercial and industrial zoning districts shall install a 10-foot buffer wall screening the property. For developments located on Commercial Boulevard an 8-foot buffer wall shall be installed. 
(Ord. No. 93-178, § 2, 11-8-93; Ord. No. 94-158, § 8, 2-13-95; Ord. No. 95-115, § 6, 3-27-95; Ord. No. 95O-155, § 3, 9-26-95; Ord. No. 97O-8-143, § 1, 9-8-97; Ord. No. 98O-6-125, § 1, 6-29-98; Ord. No. 98O-12-187, § 1, 1-11-99; Ord. No. 00O-1-9, § 1, 2-14-00; Ord. No. 01O-01-04, § 1, 2, 1-29-01; Ord. No. 02O-07-145, §§ 1—3, 8-26-02; Ord. No. 03O-02-117, § 1, 2-24-03; Ord. No. 03O-01-105, § 1, 3-31-03; Ord. No. 03O-03-129, § 1, 4-14-03; Ord. No. 05O-03-119, § 1, 3-28-05; Ord. No. 05O-03-125, § 1, 3-28-05; Ord. No. 05O-03-126, § 1, 3-28-05; Ord. No. 05O-08-173, § 1, 9-12-05; Ord. No. 05O-09-189, § 1, 11-14-05; Ord. No. 06O-03-120, §§ 1, 2, 4-10-06; Ord. No. 08O-08-132, § 1(Exh. 1), 9-8-08; Ord. No. 13O-01-105, § 10(Exh. 1), 1-28-2013; Ord. No. 13O-08-132, § 1(Exh. 1), 10-28-2013; Ord. No. 23O-06-113, § 5, 6-26-2023)
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