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MCC III Shell Building and Utilities


Ceiling eave height – 36’

Column spacing – 33’4”
· [bookmark: _GoBack]Post span – 33’4”
· Bay span – 83’4”

Storefront- 25% glass 

Dock door (1) – 8’x10’
· Building designed to accommodate up to 2 additional framed dock doors

Drive-in door (1) – 12’x14’

Personnel doors – 6 (1-Main front door)

Floor - Subgrade is set up at 8" (below finished floor). 

Basic build-out timeframe – 4 to 5 months

Water - Town of Middlesex- 8" main

Sewer - Town of Middlesex 8” gravity sewer

Electric - Duke Energy 3-phase underground along parkway
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Nash County
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