[bookmark: R-8_URBAN_MULTIFAMILY_RESIDENTIAL_CLASSI]R-8 URBAN MULTIFAMILY RESIDENTIAL CLASSIFICATION*
 
*Editor's note:  Section 21 of Ord. No. 90-34, adopted Sept. 27, 1990, added the word "Urban" to the R-8 classification. 
Purpose and intent:  The purpose and intent of the R-8 Urban Multifamily Residential Classification is to provide for multifamily residential projects in urban areas of the county. 
Permitted principal uses and structures:  In the R-8 Urban Multifamily Residential Classification, no premises shall be used except for the following uses and their customary accessory uses or structures: 
Communication towers not exceeding 70 feet in height above ground level.
Community residential home (refer to subsection 72-290(3)).
Essential utility services.
Exempt excavations (refer to subsection 72-293(15)) and/or those which comply with division 8 of the Land Development Code of Volusia County [article III] and/or final site plan review procedures of this article.
Exempt landfills (refer to section 72-293(16)).
Fire stations.
Home occupations, class A (refer to section 72-283).
Houses of worship.
Multifamily standard or manufactured modular dwellings, [town houses].*
*Note--Bracketed text omitted in Ord. No. 84-1, § XVI. See the editor's note to the R-7 classification.
Parks and recreation areas accessory to residential developments.
Public schools.
Publicly owned parks and recreational areas.
Publicly owned or regulated water supply wells.
Permitted special exceptions:  Additional regulations/requirements governing permitted special exceptions are located in sections 72-293 and 72-415 of this article. 
Boat docks containing more than 500 square feet of over-water surface area when said docks are located in outstanding Florida waters, as authorized under F.S. § 403.061, or more than 1,000 square feet of over-water surface area when said docks are not located in outstanding Florida waters.
Cemeteries (refer to subsection 72-293(4)).
Communication towers exceeding 70 feet in height above ground level.
Day care centers (refer to subsection 72-293(6)).
Dogs and cats boarded as personal pets exceeding the number permitted in subsection 72-306(a).
Excavations only for stormwater retention ponds for which a permit is required by this article.
Group home (refer to subsection 72-293(12)).
Nursing homes, boardinghouses approved and licensed by the appropriate state agency (refer to subsection 72-293(12)).
Off-street parking areas (refer to subsection 72-293(15)).
Public uses not listed as a permitted principal use.
Public uses and utilities (refer to subsections 72-293(1), (2)).
Public utility uses and structures (refer to subsection 72-293(1)).
Recreational areas (refer to subsection 72-293(3)).
Schools, parochial and private (refer to subsection 72-293(4)).
Dimensional requirements:   
Minimum lot size:   
Area: 10,000 square feet.
Width: 100 feet.
Maximum density:  20 dwellings per net acre of land. 
Minimum yard size:   
Front yard: 25 feet, except on a corner lot, one front yard may be reduced to 20 feet.
Side yard: 12 feet.
Rear yard: 25 feet.
(Buildings over 25 feet in height shall provide additional interior side yards and rear yards at a ratio of one foot of yard for every foot of building height over 25 feet.)
Waterfront yard:
On river, canal or lake: 25 feet.
On ocean: 25 feet as measured from the seawall line or the seaward limit of the permanent vegetation.
Minimum floor area:   
Studio or efficiency: 480 square feet.
One bedroom: 575 square feet.
Each additional bedroom: 150 square feet.
Maximum building length and width:  No building shall exceed 200 feet in length or width. 
Minimum building separation requirements:  50 feet between fronts or rears of principal buildings, and 25 feet between any other combination of principal building arrangements. 
Minimum building setback from streets and drives:  No principal building shall be located closer than ten feet from any interior street, drive or off-street parking area; however, this requirement shall not apply to an off-street parking area which is under a principal building. (On lots with a width or depth of less than 135 feet, the minimum principal building setback from interior streets, drives and parking areas shall be five feet.) 
Maximum building height:  45 feet. 
Off-street parking and loading requirements:  Off-street parking and loading areas meeting the requirements of sections 72-286 and 72-287 shall be constructed. 
Landscape buffer requirements:  A landscaped buffer area meeting the requirements of section 72-284 shall be constructed. 
Final site plan requirements:  Final site plan approval meeting the requirements of division 3 of the Land Development Code [article III] is required. 
(Ord. No. 81-39, § XVI, 11-19-81; Ord. No. 82-20, § XIII, 12-9-82; Ord. No. 84-1, §§ III, VII, XVI, 3-8-84; Ord. No. 85-2, § I, 3-14-85; Ord. No. 85-24, § VII, 10-10-85; Ord. No. 87-14, § III, IV, 6-18-87; Ord. No. 87-25, § III, 9-10-87; Ord. No. 88-2, § IV, 1-19-88; Ord. No. 89-20, §§ VI, VII, 6-20-89; Ord. No. 90-34, § 21, 9-27-90; Ord. No. 92-6, § XXIII, 6-4-92; Ord. No. 94-4, § XXV, 5-5-94; Ord. No. 97-19, § II, 8-7-97; Ord. No. 98-25, § VII, 12-17-98; Ord. No. 2004-20, § V, 12-16-04; Ord. No. 2009-17, § III, 5-21-09)
 

