Warm Vanilla Box 
• 4 Interior Perimeter Walls Sheetrocked, Sanded and Primed (ready for Tenant to Paint). 
• Includes one (1) ADA compliant restroom built to code with toilet, sink, working plumbing and 5 
gallon hot water heater for sink (usually located in the ceiling above the restroom). 
• Drop down acoustical panel ceiling (if Tenant wants an open ceiling it can happen, but it will cost 
them more and the difference is at their own expense) 
• Concrete Floor, sealed (ready for Tenant to address from there at their own expense) *No extra 
plumbing or electrical in the floor itself. Only plumbing included is to/from the restroom. 
• HVAC Fully Installed and Operational including ductwork, vents, returns - rated for a Retail Environment. 
1. Open Ceiling Ductwork will cost more but Tenant is responsible for any cost difference if they elect to go that route, 
2. Uses such as restaurants, and places like Salt Marsh with a lot of coolers that put off heat need more HVAC than a retail setting and tenant is responsible for the cost difference if they need a higher HVAC tonnage. Engineered Drawings and Spec Sheets for any/all Equipment have to be submitted to the Town and they make the determination of how much extra HVAC tonnage is required) 
• Full Electrical 200 Amp Service installed to code with outlet spacings on the perimeter walls only 
per the Town of Surf City code - again for a retail environment only. Any upgrades are at the sole cost of the Tenant. 
• Basic Lighting Package installed and operational - again rated for a retail environment only. 
• Glass Storefront w/ one (1) window panel on each side of front door. *Like at Triton Village 
• Rear Metal Fire Door. 36" Wide. 
• Fire Exit Signage. Operational. 
• Hot wire to signage panel above the front of the unit. Tenants pay for all their own signs including 
their installation. 
Exceptions 
*Only exceptions to this are the eight (8) endcaps - four (4) on each floor - that have the patios or balconies - additional items needed there are:
1. outdoor lighting on the underside of the ceilings over the outdoor space and maybe wiring stubbed for Tenant to install up to three (3) ceiling fans. 
2. Electrical outlets on exterior walls to the outdoor space distributed similar to the interior outlets. 
3. Glass storefront door from inside of units to patio / balcony. 
